# Delta calibration - Klipper documentation

Skip to content

# Delta calibration

This document describes Klipper's automatic calibration system for "delta" style printers.

Delta calibration involves finding the tower endstop positions, tower angles, delta radius, and delta arm lengths. These settings control printer motion on a delta printer. Each one of these parameters has a non-obvious and non-linear impact and it is difficult to calibrate them manually. In contrast, the software calibration code can provide excellent results with just a few minutes of time. No special probing hardware is necessary.

Ultimately, the delta calibration is dependent on the precision of the tower endstop switches. If one is using Trinamic stepper motor drivers then consider enabling endstop phase detection to improve the accuracy of those switches.

## Automatic vs manual probing

Klipper supports calibrating the delta parameters via a manual probing method or via an automatic Z probe.

A number of delta printer kits come with automatic Z probes that are not sufficiently accurate (specifically, small differences in arm length can cause effector tilt which can skew an automatic probe). If using an automatic probe then first calibrate the probe and then check for a probe location bias. If the automatic probe has a bias of more than 25 microns (.025mm) then use manual probing instead. Manual probing only takes a few minutes and it eliminates error introduced by the probe.

If using a probe that is mounted on the side of the hotend (that is, it has an X or Y offset) then note that performing delta calibration will invalidate the results of probe calibration. These types of probes are rarely suitable for use on a delta (because minor effector tilt will result in a probe location bias). If using the probe anyway, then be sure to rerun probe calibration after any delta calibration.

## Basic delta calibration

Klipper has a DELTA_CALIBRATE command that can perform basic delta calibration. This command probes seven different points on the bed and calculates new values for the tower angles, tower endstops, and delta radius.

In order to perform this calibration the initial delta parameters (arm lengths, radius, and endstop positions) must be provided and they should have an accuracy to within a few millimeters. Most delta printer kits will provide these parameters - configure the printer with these initial defaults and then go on to run the DELTA_CALIBRATE command as described below. If no defaults are available then search online for a delta calibration guide that can provide a basic starting point.

During the delta calibration process it may be necessary for the printer to probe below what would otherwise be considered the plane of the bed. It is typical to permit this during calibration by updating the config so that the printer's `minimum_z_position=-5`. (Once calibration completes, one can remove this setting from the config.)

There are two ways to perform the probing - manual probing (`DELTA_CALIBRATE METHOD=manual`) and automatic probing (`DELTA_CALIBRATE`). The manual probing method will move the head near the bed and then wait for the user to follow the steps described at "the paper test" to determine the actual distance between the nozzle and bed at the given location.

To perform the basic probe, make sure the config has a [delta_calibrate] section defined and then run the tool:

    G28
    DELTA_CALIBRATE METHOD=manual

After probing the seven points new delta parameters will be calculated. Save and apply these parameters by running:

    SAVE_CONFIG

The basic calibration should provide delta parameters that are accurate enough for basic printing. If this is a new printer, this is a good time to print some basic objects and verify general functionality.

## Enhanced delta calibration

The basic delta calibration generally does a good job of calculating delta parameters such that the nozzle is the correct distance from the bed. However, it does not attempt to calibrate X and Y dimensional accuracy. It's a good idea to perform an enhanced delta calibration to verify dimensional accuracy.

This calibration procedure requires printing a test object and measuring parts of that test object with digital calipers.

Prior to running an enhanced delta calibration one must run the basic delta calibration (via the DELTA_CALIBRATE command) and save the results (via the SAVE_CONFIG command). Make sure there hasn't been any notable change to the printer configuration nor hardware since last performing a basic delta calibration (if unsure, rerun the basic delta calibration, including SAVE_CONFIG, just prior to printing the test object described below.)

Use a slicer to generate G-Code from the docs/prints/calibrate_size.stl file. Slice the object using a slow speed (eg, 40mm/s). If possible, use a stiff plastic (such as PLA) for the object. The object has a diameter of 140mm. If this is too large for the printer then one can scale it down (but be sure to uniformly scale both the X and Y axes). If the printer supports significantly larger prints then this object can also be increased in size. A larger size can improve the measurement accuracy, but good print adhesion is more important than a larger print size.

Print the test object and wait for it to fully cool. The commands described below must be run with the same printer settings used to print the calibration object (don't run DELTA_CALIBRATE between printing and measuring, or do something that would otherwise change the printer configuration).

If possible, perform the measurements described below while the object is still attached to the print bed, but don't worry if the part detaches from the bed - just try to avoid bending the object when performing the measurements.

Start by measuring the distance between the center pillar and the pillar next to the "A" label (which should also be pointing towards the "A" tower).

Then go counterclockwise and measure the distances between the center pillar and the other pillars (distance from center to pillar across from C label, distance from center to pillar with B label, etc.).

Enter these parameters into Klipper with a comma separated list of floating point numbers:

    DELTA_ANALYZE CENTER_DISTS=<a_dist>,<far_c_dist>,<b_dist>,<far_a_dist>,<c_dist>,<far_b_dist>

Provide the values without spaces between them.

Then measure the distance between the A pillar and the pillar across from the C label.

Then go counterclockwise and measure the distance between the pillar across from C to the B pillar, the distance between the B pillar and the pillar across from A, and so on.

Enter these parameters into Klipper:

    DELTA_ANALYZE OUTER_DISTS=<a_to_far_c>,<far_c_to_b>,<b_to_far_a>,<far_a_to_c>,<c_to_far_b>,<far_b_to_a>

At this point it is okay to remove the object from the bed. The final measurements are of the pillars themselves. Measure the size of the center pillar along the A spoke, then the B spoke, and then the C spoke.

Enter them into Klipper:

    DELTA_ANALYZE CENTER_PILLAR_WIDTHS=<a>,<b>,<c>

The final measurements are of the outer pillars. Start by measuring the distance of the A pillar along the line from A to the pillar across from C.

Then go counterclockwise and measure the remaining outer pillars (pillar across from C along the line to B, B pillar along the line to pillar across from A, etc.).

And enter them into Klipper:

    DELTA_ANALYZE OUTER_PILLAR_WIDTHS=<a>,<far_c>,<b>,<far_a>,<c>,<far_b>

If the object was scaled to a smaller or larger size then provide the scale factor that was used when slicing the object:

    DELTA_ANALYZE SCALE=1.0

(A scale value of 2.0 would mean the object is twice its original size, 0.5 would be half its original size.)

Finally, perform the enhanced delta calibration by running:

    DELTA_ANALYZE CALIBRATE=extended

This command can take several minutes to complete. After completion it will calculate updated delta parameters (delta radius, tower angles, endstop positions, and arm lengths). Use the SAVE_CONFIG command to save and apply the settings:

    SAVE_CONFIG

The SAVE_CONFIG command will save both the updated delta parameters and information from the distance measurements. Future DELTA_CALIBRATE commands will also utilize this distance information. Do not attempt to reenter the raw distance measurements after running SAVE_CONFIG, as this command changes the printer configuration and the raw measurements no longer apply.

### Additional notes

- If the delta printer has good dimensional accuracy then the distance between any two pillars should be around 74mm and the width of every pillar should be around 9mm. (Specifically, the goal is for the distance between any two pillars minus the width of one of the pillars to be exactly 65mm.) Should there be a dimensional inaccuracy in the part then the DELTA_ANALYZE routine will calculate new delta parameters using both the distance measurements and the previous height measurements from the last DELTA_CALIBRATE command.

- DELTA_ANALYZE may produce delta parameters that are surprising. For example, it may suggest arm lengths that do not match the printer's actual arm lengths. Despite this, testing has shown that DELTA_ANALYZE often produces superior results. It is believed that the calculated delta parameters are able to account for slight errors elsewhere in the hardware. For example, small differences in arm length may result in a tilt to the effector and some of that tilt may be accounted for by adjusting the arm length parameters.

## Using Bed Mesh on a Delta

It is possible to use bed mesh on a delta. However, it is important to obtain good delta calibration prior to enabling a bed mesh. Running bed mesh with poor delta calibration will result in confusing and poor results.

Note that performing delta calibration will invalidate any previously obtained bed mesh. After performing a new delta calibration be sure to rerun BED_MESH_CALIBRATE.

Back to top