Page blank
    Attributes
        ID                 : 0
        Scope              : local
        Dragging           : 0
        Send Component ID  : on press and release
        Locked             : no
        Swide up page ID   : disabled
        Swide down page ID : disabled
        Swide left page ID : disabled
        Swide right page ID: disabled
    
    Events
        Preinitialize Event
            sendme
            dim=100
            covx baud,baud_rate.txt,0,0
            baud_rate.txt+=" bps"
        
        Touch Press Event
            dim=100
            tm0.en=1
        
        Touch Release Event
            dim=100
            tm0.en=1
        
Variable (int32) counter
    Attributes
        ID   : 9
        Scope: local
        Value: 0
    
Variable (string) aux1
    Attributes
        ID            : 10
        Scope         : local
        Text          : 
        Max. Text Size: 10
    
Text file_name
    Attributes
        ID                 : 4
        Scope              : local
        Dragging           : 0
        Send Component ID  : on press and release
        Associated Keyboard: none
        Text               : nspanel_blank.tft
        Max. Text Size     : 20
    
    Events
        Touch Press Event
            dim=100
            tm0.en=1
        
        Touch Release Event
            dim=100
            tm0.en=1
        
Text baud_rate
    Attributes
        ID                 : 5
        Scope              : local
        Dragging           : 0
        Send Component ID  : on press and release
        Associated Keyboard: none
        Text               : 
        Max. Text Size     : 20
    
    Events
        Touch Press Event
            dim=100
            tm0.en=1
        
        Touch Release Event
            dim=100
            tm0.en=1
        
Text tft_version
    Attributes
        ID                 : 6
        Scope              : local
        Dragging           : 0
        Send Component ID  : on press and release
        Associated Keyboard: none
        Text               : TFT: v2023.12.2
        Max. Text Size     : 20
    
    Events
        Touch Press Event
            dim=100
            tm0.en=1
        
        Touch Release Event
            dim=100
            tm0.en=1
        
Text framework
    Attributes
        ID                 : 7
        Scope              : local
        Dragging           : 0
        Send Component ID  : on press and release
        Associated Keyboard: none
        Text               : 
        Max. Text Size     : 20
    
    Events
        Touch Press Event
            dim=100
            tm0.en=1
        
        Touch Release Event
            dim=100
            tm0.en=1
        
Text esp_version
    Attributes
        ID                 : 8
        Scope              : local
        Dragging           : 0
        Send Component ID  : on press and release
        Associated Keyboard: none
        Text               : ESP: Waiting...
        Max. Text Size     : 20
    
    Events
        Touch Press Event
            dim=100
            tm0.en=1
        
        Touch Release Event
            dim=100
            tm0.en=1
        
QR Code qr0
    Attributes
        ID               : 1
        Scope            : local
        Dragging         : 0
        Send Component ID: on press and release
        Text             : https://github.com/Blackymas/NSPanel_HA_Blueprint/blob/main/docs/en/nspanel_blank.md#what-to-do-after-installing-nspanel_blanktft
        Max. Text Size   : 150
    
    Events
        Touch Press Event
            dim=100
            tm0.en=1
        
        Touch Release Event
            dim=100
            tm0.en=1
        
Timer tm0
    Attributes
        ID         : 2
        Scope      : local
        Period (ms): 65500
        Enabled    : yes
    
    Events
        Timer Event
            if(dim>50)
            {
                dim=50
            }else if(dim>25)
            {
                dim=25
            }else if(dim>10)
            {
                dim=10
            }else
            {
                dim=0
                tm0.en=0
            }
        
Timer tm_esphome
    Attributes
        ID         : 3
        Scope      : local
        Period (ms): 30000
        Enabled    : yes
    
    Events
        Timer Event
            counter.val++
            if(counter.val>60)
            {
                rest
            }
            sendme
            printh 91
            prints "display_mode",0
            printh 00
            prints display_mode,0
            printh FF FF FF
            printh 92
            prints "tft_version",0
            printh 00
            prints tft_version.txt,0
            printh 00
            printh FF FF FF
            covx counter.val,aux1.txt,0,0
            esp_version.txt="ESP: Retry #"+aux1.txt
            sys0=counter.val%10
            if(sys0==0)
            {
                baud=115200
            }
            covx baud,baud_rate.txt,0,0
            baud_rate.txt+=" bps"
        
