Page cardMedia
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Locked                              : no
        Swide up page ID                    : disabled
        Swide down page ID                  : disabled
        Swide left page ID                  : disabled
        Swide right page ID                 : disabled
    
    Events
        Preinitialize Event
            dim=dimValueNormal
            vis p0,0
            vis tSend,0
            vis tInstruction,0
            vis tTmp,0
            vis tId,0
            vis t5,0
            vis bPrev,0
            vis bNext,0
            cardMedia.bco=defaultBcoColor
            for(sys0=0;sys0<34;sys0++)
            {
                if(b[sys0].type==98||b[sys0].type==116)
                {
                    b[sys0].bco=defaultBcoColor
                    b[sys0].pco=defaultFontColor
                }
            }
            if(defaultBcoColor==0)
            {
                hVolume.pic=14
                hVolume.pic1=13
                hVolume.pic2=15
            }
        
Variable (string) entn
    Attributes
        Scope         : local
        Text          : 
        Max. Text Size: 80
    
Variable (string) strCommand
    Attributes
        Scope         : local
        Text          : 
        Max. Text Size: 750
    
Variable (string) tSend
    Attributes
        Scope         : local
        Text          : 
        Max. Text Size: 200
    
Variable (string) vaMenu
    Attributes
        Scope         : local
        Text          : 
        Max. Text Size: 50
    
Variable (string) vaSpeakerList
    Attributes
        Scope         : local
        Text          : 
        Max. Text Size: 400
    
Variable (int32) vaSpeakerPos
    Attributes
        Scope: local
        Value: 0
    
Text t0
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î­
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            // event,buttonPress2,entn,media-back
            //craft command
            tSend.txt="event,buttonPress2,"
            tSend.txt+=entn.txt+","
            tSend.txt+="media-back"
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Text t1
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            hVolume.val=hVolume.val-1
            // event,buttonPress2,internalNameEntity,volumeSlider,50
            //craft command
            tSend.txt="event,buttonPress2,"+entn.txt+",volumeSlider,"
            covx hVolume.val,tTmp.txt,0,0
            tSend.txt+=tTmp.txt
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Text t2
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î¬
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            // event,buttonPress2,entn,media-next
            //craft command
            tSend.txt="event,buttonPress2,"
            tSend.txt+=entn.txt+","
            tSend.txt+="media-next"
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Text t3
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            hVolume.val=hVolume.val+1
            // event,buttonPress2,internalNameEntity,volumeSlider,50
            //craft command
            tSend.txt="event,buttonPress2,"+entn.txt+",volumeSlider,"
            covx hVolume.val,tTmp.txt,0,0
            tSend.txt+=tTmp.txt
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Text t4
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î
        Max. Text Size                      : 10
    
Text t5
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î¤
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            // event,buttonPress2,entn,media-next
            //craft command
            tSend.txt="event,buttonPress2,"
            tSend.txt+=entn.txt+","
            tSend.txt+="media-OnOff"
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Text t6
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î´
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            //speaker
            tSpeaker.pco=65535
            spstr vaSpeakerList.txt,tSpeaker.txt,"?",vaSpeakerPos.val
            vaSpeakerPos.val+=1
            if(tSpeaker.txt=="")
            {
                vaSpeakerPos.val=0
                spstr vaSpeakerList.txt,tSpeaker.txt,"?",vaSpeakerPos.val
            }
        
Text tAuthor
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 50
    
Text tHeading
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 40
    
Text tIcon
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 10
    
    Events
        Touch Release Event
            if(vaMenu.txt!="")
            {
                tSend.txt="event,buttonPress2,"+vaMenu.txt+",button"
                //send calc crc
                btlen tSend.txt,sys0
                crcrest 1,0xffff // reset CRC
                crcputh 55 bb
                crcputs sys0,2
                crcputs tSend.txt,0
                //send cmd
                printh 55 bb
                prints sys0,2
                prints tSend.txt,0
                prints crcval,2
            }
        
Text tId
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 20
    
Text tInstruction
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 20
    
Text tPlayPause
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : î£
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            // event,buttonPress2,entn,media-pause
            //craft command
            tSend.txt="event,buttonPress2,"
            tSend.txt+=entn.txt+","
            tSend.txt+="media-pause"
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Text tSpeaker
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 50
    
    Events
        Touch Press Event
            // event,buttonPress2,entn,media-next
            //craft command
            tSend.txt="event,buttonPress2,"
            tSend.txt+=entn.txt+","
            tSend.txt+="speaker-sel,"+tSpeaker.txt
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Text tTitle
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 50
    
Text tTmp
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Associated Keyboard                 : none
        Text                                : 
        Max. Text Size                      : 10
    
Picture p0
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
    
Slider hVolume
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        Position                            : 50
        Upper range limit                   : 100
        Lower range limit                   : 0
    
    Events
        Touch Release Event
            tmCooldown.en=1
            tmCooldown.tim=800
            // event,buttonPress2,internalNameEntity,volumeSlider,50
            //craft command
            tSend.txt="event,buttonPress2,"+entn.txt+",volumeSlider,"
            covx hVolume.val,tTmp.txt,0,0
            tSend.txt+=tTmp.txt
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Button bNext
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        State                               : unpressed
        Text                                : î³
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            tSend.txt="event,buttonPress2,cardMedia,"
            if(bNext.txt=="î")
            {
                tSend.txt+="bHome"
            }else
            {
                tSend.txt+="bNext"
            }
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Button bPrev
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
        State                               : unpressed
        Text                                : î°
        Max. Text Size                      : 10
    
    Events
        Touch Press Event
            tSend.txt="event,buttonPress2,cardMedia,"
            if(bPrev.txt=="î¶")
            {
                tSend.txt+="bUp"
            }else
            {
                tSend.txt+="bPrev"
            }
            //send calc crc
            btlen tSend.txt,sys0
            crcrest 1,0xffff // reset CRC
            crcputh 55 bb
            crcputs sys0,2
            crcputs tSend.txt,0
            //send cmd
            printh 55 bb
            prints sys0,2
            prints tSend.txt,0
            prints crcval,2
        
Hotspot mSwipeNext
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
    
    Events
        Touch Press Event
            click bNext,1
        
Hotspot mSwipePrev
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
    
    Events
        Touch Press Event
            click bPrev,1
        
Hotspot mSwipeUp
    Attributes
        Scope                               : local
        Dragging                            : 0
        Disable release event after dragging: 0
        Send Component ID                   : disabled
    
    Events
        Touch Press Event
            click bPrev,1
        
Timer tmCooldown
    Attributes
        Scope      : local
        Period (ms): 100
        Enabled    : no
    
    Events
        Timer Event
            tmCooldown.en=0
        
Timer tmSerial
    Attributes
        Scope      : local
        Period (ms): 50
        Enabled    : yes
    
    Events
        Timer Event
            // data available
            if(usize>1)
            {
                bufferPos=0
                while(bufferPos<usize)
                {
                    // check for 0x55 0xBB - Command Init Secuence
                    if(u[bufferPos]==187&&u[bufferPos-1]==85)
                    {
                        //remove garbage at the start of the buffer if there's any to free buffer for command
                        if(u[bufferPos]!=1)
                        {
                            udelete bufferPos-1
                        }
                        //instruction is now aligned with buffer, because we deleted garbage before instrcution
                        //get length after init sequence (check if there are more than to bytes in buffer)
                        if(3<usize)
                        {
                            // check if serial buffer has reached the announced length
                            ucopy payloadLength,2,2,0
                            // we are only checking payload length so we have to skip first 3 bytes (init+payload length) (-1 because of < instead of <=)
                            payloadLength+=3
                            // payload length does also not contain crc, so we are adding another 2 bytes for crc
                            payloadLength+=2
                            if(payloadLength<usize)
                            {
                                // calculate crc
                                crcrest 1,0xFFFF
                                // u[2] contains payload legth at 3rd pos in buffer, we are calculating crc from 3rd pos with number of bytes from payload length
                                //crcputu 3,u[2]
                                // u[2] cotnains payload length, we are calculating a crc over the whole message, so we have to add 3 to the length from u[2]
                                crcputu 0,payloadLength-1
                                // get recived crc to be able to compare it
                                ucopy recvCrc,payloadLength-1,2,0
                                // compare crc with recived value
                                if(crcval==recvCrc)
                                {
                                    // crc is okay
                                    // here is the location where acual code should be
                                    // write command to variable strCommand
                                    ucopy strCommand.txt,4,payloadLength-5,0
                                    // write instruction to tInstuction (debug output, but used as variable here, ui elements will be disabled by default)
                                    spstr strCommand.txt,tInstruction.txt,"~",0
                                    if(tInstruction.txt=="entityUpd")
                                    {
                                        //heading
                                        spstr strCommand.txt,tHeading.txt,"~",1
                                        // navigation icons
                                        spstr strCommand.txt,tId.txt,"~",2
                                        spstr tId.txt,tTmp.txt,"|",0
                                        if(tTmp.txt=="0")
                                        {
                                            vis bPrev,0
                                            tsw mSwipePrev,0
                                            tsw mSwipeUp,0
                                        }
                                        if(tTmp.txt=="1")
                                        {
                                            vis bPrev,1
                                            tsw mSwipePrev,1
                                            tsw mSwipeUp,0
                                            bPrev.txt="î°"
                                        }
                                        if(tTmp.txt=="2")
                                        {
                                            vis bPrev,1
                                            tsw mSwipePrev,0
                                            tsw mSwipeUp,1
                                            bPrev.txt="î¶"
                                        }
                                        spstr tId.txt,tTmp.txt,"|",1
                                        if(tTmp.txt=="0")
                                        {
                                            vis bNext,0
                                            tsw mSwipeNext,0
                                        }
                                        if(tTmp.txt=="1")
                                        {
                                            vis bNext,1
                                            tsw mSwipeNext,1
                                            bNext.txt="î³"
                                        }
                                        if(tTmp.txt=="2")
                                        {
                                            vis bNext,1
                                            bNext.txt="î"
                                        }
                                        //entity name
                                        spstr strCommand.txt,entn.txt,"~",3
                                        //icon
                                        spstr strCommand.txt,tIcon.txt,"~",4
                                        //icon farbe
                                        spstr strCommand.txt,tTmp.txt,"~",5
                                        if(tTmp.txt!="")
                                        {
                                            covx tTmp.txt,tIcon.pco,0,0
                                        }
                                        //title
                                        spstr strCommand.txt,tTitle.txt,"~",6
                                        //title farbe
                                        spstr strCommand.txt,tTmp.txt,"~",7
                                        if(tTmp.txt!="")
                                        {
                                            covx tTmp.txt,tTitle.pco,0,0
                                        }
                                        //author
                                        spstr strCommand.txt,tAuthor.txt,"~",8
                                        //author farbe
                                        spstr strCommand.txt,tTmp.txt,"~",9
                                        if(tTmp.txt!="")
                                        {
                                            covx tTmp.txt,tAuthor.pco,0,0
                                        }
                                        //volume
                                        spstr strCommand.txt,tTmp.txt,"~",10
                                        covx tTmp.txt,sys0,0,0
                                        hVolume.val=sys0
                                        //icon
                                        spstr strCommand.txt,tPlayPause.txt,"~",11
                                        //speaker current
                                        spstr strCommand.txt,tSpeaker.txt,"~",12
                                        if(tSpeaker.txt!="")
                                        {
                                            tSpeaker.pco=1374
                                        }else
                                        {
                                            tSpeaker.pco=65535
                                        }
                                        //speaker list
                                        spstr strCommand.txt,vaSpeakerList.txt,"~",13
                                        if(vaSpeakerList.txt=="")
                                        {
                                            vis t6,0
                                        }
                                        vaSpeakerPos.val=0
                                        // on off button
                                        spstr strCommand.txt,tTmp.txt,"~",14
                                        if(tTmp.txt=="disable")
                                        {
                                            vis t5,0
                                        }else
                                        {
                                            vis t5,1
                                            covx tTmp.txt,t5.pco,0,0
                                        }
                                        //tIconBtnEntityName
                                        spstr strCommand.txt,vaMenu.txt,"~",15
                                    }
                                    if(tInstruction.txt=="time")
                                    {
                                        // get set time to global variable
                                        spstr strCommand.txt,pageIcons.vaTime.txt,"~",1
                                    }
                                    if(tInstruction.txt=="date")
                                    {
                                        // get set date to global variable
                                        spstr strCommand.txt,pageIcons.vaDate.txt,"~",1
                                    }
                                    if(tInstruction.txt=="dimmode")
                                    {
                                        // get value
                                        spstr strCommand.txt,tTmp.txt,"~",1
                                        covx tTmp.txt,dimValue,0,0
                                        // get value normal
                                        spstr strCommand.txt,tTmp.txt,"~",2
                                        covx tTmp.txt,dimValueNormal,0,0
                                        dim=dimValueNormal
                                        // get background color
                                        spstr strCommand.txt,tTmp.txt,"~",3
                                        if(tTmp.txt!="")
                                        {
                                            covx tTmp.txt,defaultBcoColor,0,0
                                        }
                                        // get font color
                                        spstr strCommand.txt,tTmp.txt,"~",4
                                        if(tTmp.txt!="")
                                        {
                                            covx tTmp.txt,defaultFontColor,0,0
                                        }
                                    }
                                    if(tInstruction.txt=="timeout")
                                    {
                                        //set timeout to global var
                                        spstr strCommand.txt,tTmp.txt,"~",1
                                        covx tTmp.txt,sleepTimeout,0,0
                                    }
                                    if(tInstruction.txt=="pageType")
                                    {
                                        sleepValue=0
                                        //command format pageType,specialPageName
                                        //write name of speical page to tId
                                        spstr strCommand.txt,tId.txt,"~",1
                                        //save second arg if there's one
                                        spstr strCommand.txt,tTmp.txt,"~",2
                                        //save third arg if there's one
                                        spstr strCommand.txt,pageIcons.tTmp2.txt,"~",3
                                        spstr strCommand.txt,pageIcons.tTmp3.txt,"~",4
                                        //we are going to exit this page with this command, so we have to clear the buffer, so we are not getting into a stupid loop ...
                                        udelete payloadLength-1
                                        bufferPos=0
                                        if(tId.txt=="pageStartup")
                                        {
                                            page pageStartup
                                        }
                                        if(tId.txt=="screensaver")
                                        {
                                            page screensaver
                                        }
                                        if(tId.txt=="cardEntities")
                                        {
                                            page cardEntities
                                        }
                                        if(tId.txt=="cardGrid")
                                        {
                                            page cardGrid
                                        }
                                        if(tId.txt=="popupLight")
                                        {
                                            pageIcons.tTmp1.txt=tTmp.txt
                                            page popupLight
                                        }
                                        if(tId.txt=="popupShutter")
                                        {
                                            pageIcons.tTmp1.txt=tTmp.txt
                                            page popupShutter
                                        }
                                        if(tId.txt=="popupNotify")
                                        {
                                            page popupNotify
                                        }
                                        if(tId.txt=="cardThermo")
                                        {
                                            page cardThermo
                                        }
                                        if(tId.txt=="cardMedia")
                                        {
                                            page cardMedia
                                        }
                                        if(tId.txt=="cardAlarm")
                                        {
                                            page cardAlarm
                                        }
                                        if(tId.txt=="cardQR")
                                        {
                                            page cardQR
                                        }
                                        if(tId.txt=="cardPower")
                                        {
                                            page cardPower
                                        }
                                        if(tId.txt=="cardChart")
                                        {
                                            page cardChart
                                        }
                                    }
                                    // end of user code
                                    udelete payloadLength-1
                                    bufferPos=0
                                }
                            }
                        }
                    }
                    // next character
                    bufferPos++
                }
                if(bufferPos==usize)
                {
                    // copy whole buffer to t1.txt, for debugging
                    //ucopy t2.txt,0,usize,0
                    // ucopy n2.val,0,usize,0
                    // clear whole buffer
                    //code_c
                    //bufferPos=0
                }
            }
        
Timer tmSleep
    Attributes
        Scope      : local
        Period (ms): 1000
        Enabled    : yes
    
    Events
        Timer Event
            if(sleepTimeout!=0&&dimValue!=dim)
            {
                sleepValue+=1
                if(sleepTimeout<=sleepValue)
                {
                    sleepValue=0
                    dim=dimValue
                    tSend.txt="event,sleepReached,cardMedia"
                    //send calc crc
                    btlen tSend.txt,sys0
                    crcrest 1,0xffff // reset CRC
                    crcputh 55 bb
                    crcputs sys0,2
                    crcputs tSend.txt,0
                    //send cmd
                    printh 55 bb
                    prints sys0,2
                    prints tSend.txt,0
                    prints crcval,2
                }
            }
        
TouchCap tc0
    Attributes
        Scope: local
        Value: 0
    
    Events
        Touch Press Event
            sleepValue=0
        
